(footprint "ESP32-C5-WROOM-1"
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(layer "F.Cu")
	(descr "ESP32-C5-WROOM-1: Module that supports 2.4 and 5 GHz dual-band Wi-Fi 6 (802.11ax), Bluetooth ® 5 (LE), Zigbee, and Thread (802.15.4) Built around ESP32-C5 series of SoCs, 32-bit RISC-V single-core microprocessor Flash up to 32 MB Up to 22 GPIOs, rich set of peripherals")
	(tags "esp32-c5")
	(property "Reference" "REF**"
		(at 0 -15 0)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-C5-WROOM-1"
		(at 0 15.6 0)
		(layer "F.Fab")
	)
	(property "Datasheet" "https://documentation.espressif.com/esp32-c5-wroom-1_wroom-1u_datasheet_en.html"
		(at 0.25 2.5 0)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" "Module that supports 2.4 and 5 GHz dual-band Wi-Fi 6 (802.11ax), Bluetooth ® 5 (LE), Zigbee, and Thread (802.15.4) Built around ESP32-C5 series of SoCs, 32-bit RISC-V single-core microprocessor Flash up to 32 MB Up to 22 GPIOs, rich set of peripherals"
		(at 0.25 2.5 0)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "Antenna Area"
		(at 0.25 -10.25 0)
		(layer "F.SilkS")
	)
	(fp_text user "Antenna Area"
		(at 0.25 -10.25 0)
		(layer "Eco2.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0.25 2.5 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.5 -5.76)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "2" smd rect
		(at -8.5 -4.49)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "3" smd rect
		(at -8.5 -3.22)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "4" smd rect
		(at -8.5 -1.95)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "5" smd rect
		(at -8.5 -0.68)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "6" smd rect
		(at -8.5 0.59)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "7" smd rect
		(at -8.5 1.86)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "8" smd rect
		(at -8.5 3.13)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "9" smd rect
		(at -8.5 4.4)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "10" smd rect
		(at -8.5 5.67)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "11" smd rect
		(at -8.5 6.94)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "12" smd rect
		(at -8.5 8.21)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "13" smd rect
		(at -8.5 9.48)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "14" smd rect
		(at -8.5 10.75)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "15" smd rect
		(at 9 10.75 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "16" smd rect
		(at 9 9.48 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "17" smd rect
		(at 9 8.21 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "18" smd rect
		(at 9 6.94 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "19" smd rect
		(at 9 5.67 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "20" smd rect
		(at 9 4.4 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "21" smd rect
		(at 9 3.13 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "22" smd rect
		(at 9 1.86 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "23" smd rect
		(at 9 0.59 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "24" smd rect
		(at 9 -0.68 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "25" smd rect
		(at 9 -1.95 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "26" smd rect
		(at 9 -3.22 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "27" smd rect
		(at 9 -4.49 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "28" smd rect
		(at 9 -5.76 180)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -0.6202 1.128 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -0.6202 2.828 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at -0.6202 4.528 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 1.0798 1.128 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 1.0798 2.828 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 1.0798 4.528 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.7798 1.128 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.7798 2.828 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(pad "29" smd rect
		(at 2.7798 4.528 180)
		(size 1.3 1.3)
		(layers "F.Cu" "F.Mask" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "B.Cu" "In1.Cu" "In2.Cu" "In3.Cu" "In4.Cu" "In5.Cu" "In6.Cu"
			"In7.Cu" "In8.Cu" "In9.Cu" "In10.Cu" "In11.Cu" "In12.Cu" "In13.Cu" "In14.Cu"
			"In15.Cu" "In16.Cu" "In17.Cu" "In18.Cu" "In19.Cu" "In20.Cu" "In21.Cu"
			"In22.Cu" "In23.Cu" "In24.Cu" "In25.Cu" "In26.Cu" "In27.Cu" "In28.Cu"
			"In29.Cu" "In30.Cu"
		)
		(name "antenna keepout")
		(hatch edge 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(placement
			(enabled no)
			(sheetname "")
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy 9.25 -7.25) (xy -8.75 -7.25) (xy -8.75 -13.75) (xy 9.25 -13.75)
			)
		)
	)
	(embedded_fonts no)
	(model "${KICAD9_3RD_PARTY}/3dmodels/com_github_espressif_kicad-libraries/espressif.3dshapes/esp32-c5-wroom-1.step"
		(offset
			(xyz -8.75 -13.75 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz -0 -0 -0)
		)
	)
)
