(footprint "ESP32-S2-MINI-1" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "ESP32-S2-MINI-1 and ESP32-S2-MINI-1U: https://www.espressif.com/sites/default/files/documentation/esp32-s2-mini-1_esp32-s2-mini-1u_datasheet_en.pdf")
  (tags "ESP32-S2")
  (attr smd)
  (fp_text reference "REF**" (at 0 -13.4) (layer "F.SilkS"))
  (fp_text value "ESP32-S2-MINI-1" (at 0 9.4) (layer "F.Fab"))
  (fp_text user "Antenna Area" (at 0 -10.45) (layer "F.SilkS"))
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
  (pad "1" smd rect (at -7 -5.95 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -7 -5.1 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -7 -4.25 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -7 -3.4 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -7 -2.55 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -7 -1.7 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -7 -0.85 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -7 0 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -7 0.85 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -7 1.7 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -7 2.55 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -7 3.4 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -7 4.25 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -7 5.1 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -7 5.95 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -5.95 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at -5.1 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at -4.25 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at -3.4 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at -2.55 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at -1.7 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at -0.85 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 0 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 0.85 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 1.7 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 2.55 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 3.4 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 4.25 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 5.1 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 5.95 7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 7 5.95 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 7 5.1 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 7 4.25 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 7 3.4 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 7 2.55 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at 7 1.7 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "37" smd rect (at 7 0.85 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "38" smd rect (at 7 0 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "39" smd rect (at 7 -0.85 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "40" smd rect (at 7 -1.7 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "41" smd rect (at 7 -2.55 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "42" smd rect (at 7 -3.4 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "43" smd rect (at 7 -4.25 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "44" smd rect (at 7 -5.1 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "45" smd rect (at 7 -5.95 90) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "46" smd rect (at 5.95 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "47" smd rect (at 5.1 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "48" smd rect (at 4.25 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "49" smd rect (at 3.4 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "50" smd rect (at 2.55 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "51" smd rect (at 1.7 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "52" smd rect (at 0.85 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "53" smd rect (at 0 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "54" smd rect (at -0.85 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "55" smd rect (at -1.7 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "56" smd rect (at -2.55 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "57" smd rect (at -3.4 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "58" smd rect (at -4.25 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "59" smd rect (at -5.1 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "60" smd rect (at -5.95 -7) (size 0.4 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "61" smd custom (at -1.65 -1.65) (size 0.6 0.6) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2) (thermal_bridge_angle 45)
    (options (clearance outline) (anchor rect))
    (primitives
      (gr_poly
        (pts
          (xy 0.6 0.6)
          (xy -0.6 0.6)
          (xy -0.6 0)
          (xy 0 -0.6)
          (xy 0.6 -0.6)
        )
        (width 0) (fill yes))
    ))
  (pad "61" smd rect (at -1.65 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at -1.65 1.65) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at 0 -1.65) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at 0 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at 0 1.65) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at 1.65 -1.65) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at 1.65 0) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "61" smd rect (at 1.65 1.65) (size 1.2 1.2) (layers "F.Cu" "F.Paste" "F.Mask")
    (zone_connect 2))
  (pad "62" smd rect (at -7 -7 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "63" smd rect (at -7 7 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "64" smd rect (at 7 7 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "65" smd rect (at 7 -7 180) (size 0.8 0.8) (layers "F.Cu" "F.Paste" "F.Mask"))
  (zone (net 0) (net_name "") (layers "*.Cu") (name "antenna keepout") (hatch edge 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254) (filled_areas_thickness no)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed) (copperpour not_allowed) (footprints not_allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 7.7 -7.7)
        (xy -7.7 -7.7)
        (xy -7.7 -12.3)
        (xy 7.7 -12.3)
      )
    )
  )
  (model "${KICAD8_3RD_PARTY}/3dmodels/com_github_espressif_kicad-libraries/espressif.3dshapes/ESP32-S2-MINI-1.STEP"
    (offset (xyz -7.7 -7.7 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
